Update to 3.0.18
(from 3.0.11)

On our own behalf:
There are also Mac OS X (10.8.x, 10.9.x and 10.10.x) and Linux (Ubuntu 12.04LTS, Oracle 6.5) versions of the UTN Manager available and downloadable at http://www.seh-technology.com/services/downloads.html

Update Note:
"Administrator privileges required for installation"

Important Note:
For all fixes and improvements to work properly with your myUTN devices at least the following firmware/software combination is required:

myUTN-80(HW 1.0):
-----------------
b-fw-ps-22.bin / b-sw-uds-14.3.3.bin

myUTN-50a/250/800 and myUTN-80(HW 2.0):
---------------------------------------
r-fw-uds-14.bin / r-sw-uds-14.3.6.bin

myUTN-55:
---------
r-fw-wlan-4.bin / r-sw-uds-14.3.6.bin

The current myUTN Software can be downloaded from http://www.seh-technology.com/services/downloads.html


General Changes:
################
- Contains several bugfixes and enhancements.


Fixes/Improvements:
###################
- If the SEH UTN Manager is started for the second time, the window of the SEH UTN Manager which is already running now appears instead of an error message.
- Fixed: The 'Printer Maintainance Tool' for Epson SL-DL700 does not work with SEH UTN Manager.
- Fixed: Handle leak caused by non-closed mutex handle. The number of open handles now is stable.
- Fixed: Faulty data transmission from Apple iPhones (bulk transfers with data bigger than 65k have been by processed incorrectly by the driver)
- SEH UTN Manager also used the VirtualStore of the Microsoft Registry. The manifest was changed so that the VirtualStore of the registry can no longer be written to.
Devices connected via myUTN functionality are now displayed in USB View and USBTreeView. In addition, the following IOCTLs directed to the host controller and hub are answered now:
IOCTL_USB_GET_NODE_INFORMATION
IOCTL_USB_GET_HUB_CAPABILITIES
IOCTL_USB_GET_HUB_CAPABILITIES_EX
IOCTL_USB_GET_NODE_CONNECTION_INFORMATION_EX
IOCTL_USB_GET_NODE_CONNECTION_DRIVERKEY_NAME
IOCTL_USB_GET_DESCRIPTOR_FROM_NODE_CONNECTION
IOCTL_USB_GET_ROOT_HUB_NAME
IOCTL_GET_HCD_DRIVERKEY_NAME
IOCTL_USB_USER_REQUEST (USBUSER_GET_ROOTHUB_SYMBOLIC_NAME)


New Devices:
############
- MCU boards by Silicon Labs now are supported

Visit the SEH Computertechnik GmbH Homepage (http://www.seh-technology.com) to learn more about Products, Update information, tips, hints & more...